CORRIGENDUM No: 1

to the

Bidding document for

Procurement of services related to:

PREPARATION OF THE PRELIMINARY DESIGN AND MAIN DESIGN
OF THE NEWLY DESIGNED ELEMENTARY SCHOOL BUILDING 
IN PODGORICA

No. 24-603/26-4924/1

ICB Issued on 12th June 2026

[bookmark: _GoBack]Corrigendum issued on 17th June 2026


As a result of the clarification process the Contracting Authority makes the following modifications to the Tender Dossier:
MODIFICATION NO.1 
Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 1. Introductory part:

“Within the program “Improvement of Montenegrin Education”, financed by a loan from the European Investment Bank (EIB), there is a plan to construct a new elementary school in Zabjelo, Municipality of Podgorica.
              This project aims to enhance public educational infrastructure through the construction and renovation of kindergartens, elementary schools, high schools, and vocational schools. It also includes the procurement of modern information and communication technology (ICT), new school furniture, as well as specialized equipment for vocational schools.
Facility: Elementary School: the ground floor level + one floor (P+1)….”
has been amended as follows:
Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 1. Introductory part:

“Within the program “Improvement of Montenegrin Education”, financed by a loan from the European Investment Bank (EIB), there is a plan to construct a new elementary school in Zabjelo, Municipality of Podgorica.
              This project aims to enhance public educational infrastructure through the construction and renovation of kindergartens, elementary schools, high schools, and vocational schools. It also includes the procurement of modern information and communication technology (ICT), new school furniture, as well as specialized equipment for vocational schools.
The cadastral parcels that form part of urban planning parcel UP D1.1 parcel and owned by Montenegro are as follows:

· Cadastral parcel No. 3582/2, classified by use as a Class 5 meadow, with an area of 127 m², recorded in Real Estate Folio No. 3217, Cadastral Municipality (CM) Podgorica III; 
· Cadastral parcel No. 3693/22, classified by use as unclassified roads, with an area of 826 m², recorded in Real Estate Folio No. 720, CM Podgorica III; 
· Cadastral parcel No. 3704/1, classified by use as a Class 3 meadow, with an area of 10,561 m², recorded in Real Estate Folio No. 5973, CM Podgorica III; 
· Cadastral parcel No. 3705, classified by use as a Class 3 arable field, with an area of 1,311 m², recorded in Real Estate Folio No. 5973, CM Podgorica III.
FACILITY: Elementary School: the ground floor level + one floor (P+1)….”

MODIFICATION NO.2
[bookmark: _Toc135034975][bookmark: _Toc162963149][bookmark: _Toc168575739]Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 2.2. Elements to Design:

		Assigned urban parameters on UP D1.1	

	Intended Use
	Elementary School

	Urban Plot Designation
	UP D1.1

	Urban plot surface
	23,299.99 m².

	Maximum Site Coverage Index
	0.4

	Maximum Floor Area Ratio
	0.8

	Maximum Building Footprint Area (UT Conditions)
	9,320m²

	Maximum Gross Construction Area of Buildings (UT Conditions)
	18,640m²

	Number of Floors
	Po+P+1

	Derived Parameters

	Maximum Required Gross Construction Area of Buildings
	8100m²

	Entrance Plaza Area
	≈ 400 m²

	Parking and Service Zone Area (parking lots, kiss and ride, delivery, waste collection, maneuvering area)
	≈ 1,200 m²

	min. Area of Open Courtyard Spaces (school courtyard, sports courts, green areas, outdoor teaching facilities)
	12,400m²

	Building Capacities

	Number of Students (total)
	1240

	Number of Students per Shift
	620

	Number of Classes (total)
	44

	Number of Classes per Shift
	22

	Number of Students per Class
	26-28

	Number of Grades
	9

	Number of Employees per Shift
	50



has been replaced by the following:
		Assigned urban parameters on UP D1.1	

	Intended Use
	Elementary School

	Urban Plot Designation
	UP D1.1

	Urban plot surface
	23,299.99 m².

	Maximum Site Coverage Index
	0.4

	Maximum Floor Area Ratio
	0.8

	Maximum Building Footprint Area (UT Conditions)
	9,320m²

	Maximum Gross Construction Area of Buildings (UT Conditions)
	18,640m²

	Number of Floors
	Po+P+1

	The prescribed urban planning parameters for part of Urban Plot D1.1, comprising cadastral parcels No. 3582/2, 3693/22, 3704/1, and 3705.

	Intended Use
	Elementary School

	Designation of the Urban Plot and Cadastral Parcels
	UP D1.1, KP 3582/2, KP 3693/22, KP 3704/1, KP 3705

	Area of the Portion of Urban Plot D1.1, Consisting of Cadastral Parcels No. 3582/2, 3693/22, 3704/1, and 3705
	12825,00 m²

	Maximum Site Coverage Index
	0,4

	Maximum Floor Area Ratio
	0,8

	Maximum Building Footprint Area 
	5130,00 m²

	Maximum Permitted Gross Construction Area (Maximum GCA Includes Usable Flat Roofs and Terraces)
	10260,00 m²

	Number of Floors
	Po+P+2

	As built Parameters

	Expected Gross Floor Area of the Buildings (excluding terraces and accessible flat-roof areas)
	8100m²

	Building Capacities

	Number of Students (total)
	1240

	Number of Students per Shift
	620

	Number of Classes (total)
	44

	Number of Classes per Shift
	22

	Number of Students per Class
	26-28

	Number of Grades
	9

	Number of Employees per Shift
	50



MODIFICATION NO.3
Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 1.3:
“1.3. Bases for the preparation of technical documentation provided by the Investor
Bases for the preparation of technical documentation:
•	Terms of Reference
•	Urban-Technical Requirements numbered 06-333/24-10971/6 and dated 28/10/2024, , issued by the Ministry of Spatial Planning, Urbanism and State Property
•	A document containing specific recommendations related to the positive impact on climate change: “Climate Risk and Vulnerability Assessment for the Project ‘Montenegro Education Programme’”.
•	Rulebook on Detailed Conditions for the Establishment of Institutions in the Field of Education and Upbringing ("Official Gazette of Montenegro", No. 42/26 of March 25, 2026)”

has been amended as follows:
Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 1.3:
“1.3. Bases for the preparation of technical documentation provided by the Investor
Bases for the preparation of technical documentation:
•	Terms of Reference
•	Urban-Technical Requirements numbered 06-333/24-10971/6 and dated 28/10/2024, issued by the Ministry of Spatial Planning, Urbanism and State Property
•	A document containing specific recommendations related to the positive impact on climate change: “Climate Risk and Vulnerability Assessment for the Project ‘Montenegro Education Programme’”.
•	Rulebook on Detailed Conditions for the Establishment of Institutions in the Field of Education and Upbringing.”

MODIFICATION NO.4
Original text given under the Section VII – Terms of Reference, Technical part of the Terms of Reference, point 2.4:

[bookmark: _Toc230941387]2.4. Functional Aspects
	The elementary school shall be designed as a modern and functional facility for 620 children in one shift, or 1240 children in two shifts. 
	The facility shall be a contemporary structure, aligned with its purpose, achievable through its external appearance, functional design, and the impression created by its interior spaces. 
	When preparing the project documentation, to better understand the educational system and ensure the appropriate spatial organization of the newly planned school in Podgorica, it is necessary to thoroughly study the Rulebook on Detailed Conditions for the Establishment of Institutions in the Field of Education and Upbringing ("Official Gazette of Montenegro", No. 42/26 of March 25, 2026). With this rulebook, among other things, within the school premises, certain units are recognized in a functional sense, namely: classrooms, common rooms and other spaces. To comprehend the spatial organization, special attention shall be given to Articles 78-91.
	The clear height of all teaching rooms, ensuring adequate air volume, is a minimum of 3 meters, except for the hall for physical education (which requires a minimum clear height of 7 meters).

has been amended as follows:
“2.4. Functional Aspects
The elementary school shall be designed as a modern and functional facility for 620 children in one shift, or 1240 children in two shifts. 
The facility shall be a contemporary structure, aligned with its purpose, achievable through its external appearance, functional design, and the impression created by its interior spaces. 
When preparing the project documentation, to better understand the educational system and ensure the appropriate spatial organization of the newly planned school in Podgorica, it is necessary to thoroughly study the Rulebook on Detailed Conditions for the Establishment of Institutions in the Field of Education and Upbringing. With this rulebook, among other things, within the school premises, certain units are recognized in a functional sense, namely: classrooms, common rooms and other spaces. To comprehend the spatial organization, special attention shall be given to Articles 78-91.
	The clear height of all teaching rooms, ensuring adequate air volume, is a minimum of 3 meters, except for the hall for physical education (which requires a minimum clear height of 7 meters).”
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